**Department of Civil Engineering**

1. Bhattacharyya, S. & Sahoo, S. Stress analysis of trapezoidal nanobeam with roughness. Int. J. Mater. Manuf. Des.2, 29–44 (2014).
2. Chowdhury, Puja B. Mitra, Anirban Sahoo, S. Relative performance of antisymmetric angle-ply laminated stiffened hypar shell roofs with cutout in terms of static behavior. Curved Layer. Struct.3, 22–46 (2016).
3. Dutta, D., Bhattacharyya, S. & Sahoo, S. Effect of fractal parameters on response of nanobeam: a finite element approach. J. Nanosci. Nanoeng.1, 162–170 (2015).
4. Goswami, S., Sarkar, S. & Mazumder, D. A new approach for development of kinetics of wastewater treatment in aerobic biofilm reactor. Appl. Water Sci. 1–7 (2016).
5. Sahoo, S. Clamped saddle shells of laminated composites: Effect of cutout on natural frequency and mode shapes. Int. J. Adv. Mater. Res.1, 25–31 (2015).
6. Sahoo, S. Composite hypar shell roofs with stiffeners under point load: Optimization of stiffener arrangement. Int. J. Adv. Civ. Eng.2, 45–54 (2012).
7. Sahoo, S. Deflection and stress resultants of composite hypar shell roofs under point load and complex boundary conditions. Int. J. Sustain. Civ. Eng.4, 115–121 (2012).
8. Sahoo, S. Dynamic Characters of Stiffened Composite Conoidal Shell Roofs with Cutouts: Design Aids and Selection Guidelines. J. Eng. Article ID 230120 (2013). doi:10.1155/2013/230120
9. Sahoo, S. Finite element based analysis of nanobeam with fractal roughness. Int. J. Appl. Eng. Res.9, 8703–8706 (2014).
10. Sahoo, S. Free vibration behavior of laminated composite stiffened elliptic paraboloidal shell panel with cutout. Curved Layer. Struct.2, 162–182 (2015).
11. Sahoo, S. Laminated composite hypar shell roofs with stiffeners: Free vibration behavior under different boundary conditions. Int. J. Civ. Eng.4, 181–191 (2012).
12. Sahoo, S. Laminated composite stiffened cylindrical shell panels with cutouts under free vibration. Int. J. Manuf. Mater. Mech. Eng.5, 37–63 (2015).
13. Sahoo, S. Laminated composite stiffened elliptic paraboloid shell with cutout under clamped condition. Int. J. Civ. Eng. 5, 86-95 (2015).
14. Sahoo, S. Laminated composite stiffened saddle shells with cutouts under free vibration– a finite element approach. Adv. Mater. Manuf. Charact.4, 111–124 (2014).
15. Sahoo, S. Laminated composite stiffened shallow spherical panels with cutouts under free vibration – a finite element approach. Eng. Sci. Technol. An Int. J.17, 247–259 (2014).
16. Sahoo, S. Natural frequencies and mode shapes of clamped stiffened composite conoids with cutouts. Int. J. Adv. Civ. Eng. Archit.2, 11–26 (2014).
17. Sahoo, S. Performance evaluation of free vibration of laminated composite stiffened hyperbolic paraboloid shell panel with cutout. Int. J. Eng. Technol.7, 1–24 (2016).
18. Sahoo, S. Point supported composite stiffened saddle shells with cutouts: natural frequency and mode shapes. Int. J. Adv. Civ. Eng. Archit.2, 45–56 (2014).
19. Sahoo, S. Relative Performance of Laminated Composite Doubly Curved Shell Roofs with Cutout. Int. J. Mater. Chem. Phys.2, 15–21 (2016).
20. Sahoo, S. Some studies on composite stiffened skewed hypars under free vibration. Int. J. Mater. Manuf. Des.2, 69–78 (2014).
21. Sarkar, S. & Mazumder, D. A novel approach to modelling of an aerobic hybrid bioreactor treating easily biodegradable substances. The Global Journal of Environmental Science and Research 2, 500-504 (2015).
22. Sarkar, S. & Mazumder, D. Development of a simplified biofilm model. Appl. Water Sci. 1–8 (2015). doi:10.1007/s13201-015-0353-4
23. Sarkar, S. & Mazumder, D. Development of a simplified Model for Completely Mixed Biofilm Reactor. Water Environment Research. 12, 1601-1610 (2015).
24. Sarkar, S. & Mazumder, D. Development of a simplified model for the fixed biofilm reactor. Water Sci. Technol.72, 1601–1610 (2015).
25. Sarkar, S. & Mazumder, D. Feasibility of Hybrid Bioreactor in the treatment of wastewater containing slowly biodegradable substances. International Journal of Environmental Sciences5, 1-19 (2014).
26. Sarkar, S. & Mazumder, D. Solid waste management in steel industry-challanges and opportunity. International Journal of Chemical,Nuclear, Materialsand Metallurgical Engineering, World Academy of Science, Engineering and Technology 9, 978-981 (2015).
27. Sarkar, S. Treatability study of paint manufacturing wastewater by physico- chemical methods. Indian Journal of Environmental Protection26, 1083-1089 (2006)