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problem. The time complexity of the latter algorithm is O((n+k)=T), where T is the n @ A ()

Related  Details

total number of terminals attached to all nets in the floorplan. Solutions to these
problems are useful in modeling the repeater block placement that arises in

interconnect-driven floorplanning for deep-submicron VLSI ph

cal design. It is also

an important problem in context to the classical global routing, where channels are

used as routing space on silicon.
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